| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__GetBwUsageForGToGCACPolicyRequest Struct Reference
Call Admission Control

Get Bandwidth Usage for Group to Group CAC Policy request. More...

`#include <osv-if-doc.h>`

## Public Attributes
xsd__string | OperatorId
| Operator Id. More...
xsd__string | CACGroup1Name
| The name of the first CAC Group for this policy whose bandwidth usage information is to be retrieved. More...
xsd__string | CACGroup2Name
| The name of the second CAC Group for this policy. More...
xsd__short | CACPolicyType
| Indicates the CAC policy type. More...

## Detailed Description

Get Bandwidth Usage for Group to Group CAC Policy request.

Used by unsp__GetBwUsageForGToGCACPolicy()

## Member Data Documentation

## ◆ CACGroup1Name

xsd__string unsp__GetBwUsageForGToGCACPolicyRequest::CACGroup1Name

The name of the first CAC Group for this policy whose bandwidth usage information is to be retrieved.

required: true

See also
  unsp__CGName

## ◆ CACGroup2Name

xsd__string unsp__GetBwUsageForGToGCACPolicyRequest::CACGroup2Name

The name of the second CAC Group for this policy.

required: true

See also
  unsp__CGName

## ◆ CACPolicyType

xsd__short unsp__GetBwUsageForGToGCACPolicyRequest::CACPolicyType

Indicates the CAC policy type.

Policy type is a bitmap, where its bits represent the FaxPolicy, VoicePolicy, and VideoPolicy.

- 0x0004 (VideoPolicyType)
- 0x0005 (Voice & VideoPolicyType)
- 0x0006 (FaxPolicyType)
- 0x0007 (all three of the above)

required: true
default value[range]: NA

## ◆ OperatorId

xsd__string unsp__GetBwUsageForGToGCACPolicyRequest::OperatorId

Operator Id.

See also
  unsp__OperatorId

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h