| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__ModifyCommunityGroupRequest Struct Reference
Community Group

Modify Community Group request. More...

`#include <osv-if-doc.h>`

## Public Attributes
xsd__string | OperatorId
| Operator Id. More...
xsd__string | SubscriberDN
| The subscriber that the community group is assigned to. More...
xsd__int * | PeriodicTone
| The interval of the periodic tone in seconds used to indicate that an intercom call is active. More...

## Detailed Description

Modify Community Group request.

Used by unsp__ModifyCommunityGroup()

## Member Data Documentation

## ◆ OperatorId

xsd__string unsp__ModifyCommunityGroupRequest::OperatorId

Operator Id.

See also
  unsp__OperatorId

## ◆ PeriodicTone

xsd__int* unsp__ModifyCommunityGroupRequest::PeriodicTone

The interval of the periodic tone in seconds used to indicate that an intercom call is active.

The periodic tone applies to all terminating two-way Intercom Calls.
required: false
default value[range]: 120 [0 (none), 5..180]

## ◆ SubscriberDN

xsd__string unsp__ModifyCommunityGroupRequest::SubscriberDN

The subscriber that the community group is assigned to.

required: true

See also
  unsp__ServiceId

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h