| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__DynamicCACPolicyInfo Struct Reference
Call Admission Control

Dynamic CAC Policy Information. More...

`#include <osv-if-doc.h>`

## Public Attributes
xsd__short * | SecondaryCallLimit
| Specifies the secondary Call Limit capacity. More...
xsd__int * | SecondaryBandWidthLimit
| Specifies the secondary Bandwidth Limit capacity. More...

## Detailed Description

Dynamic CAC Policy Information.

## Member Data Documentation

## ◆ SecondaryBandWidthLimit

xsd__int* unsp__DynamicCACPolicyInfo::SecondaryBandWidthLimit

Specifies the secondary Bandwidth Limit capacity.

This parameter has the same validations as the BandWidthLimit parameter with respect to the CACPolicyLimitType. It can be entered only if the CACGroup has a RouterIPAddress configured. This parameter is mandatory if the RouterIPAddress in the CACGroup has been configured and the CACPolicyType is "BandwidthLimit" or "Both".
required: false
default value[range]: false

## ◆ SecondaryCallLimit

xsd__short* unsp__DynamicCACPolicyInfo::SecondaryCallLimit

Specifies the secondary Call Limit capacity.

This parameter has the same validations as the CallLimit parameter with respect to the CACPolicyLimitType. It can be entered only if the CACGroup has a RouterIPAddress configured. This parameter is mandatory if the RouterIPAddress in the CACGroup has been configured and the CACPolicyType is "CallLimit" or "Both".
required: false
default value[range]: false

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h