| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__ActiveDeviceDataEntry Struct Reference
CSTA Application

Active device data entry. More...

`#include <osv-if-doc.h>`

## Public Attributes
xsd__string | DeviceId
| For Subscriber Devices: If the application type is Telefonica then the Service ID is returned in EID+ExtensionFormat. More...
xsd__string | EBGId
| The EBGID. More...
xsd__boolean | Monitor
| Indicates whether this device has active monitors for the CSTA application. More...
xsd__boolean | RouteRegistration
| Indicates whether this device has active Route Registrations for the CSTA application. More...
enum unsp__CSTADeviceType | Type
| Indicates whether this device is a Subscriber or NID. More...

## Detailed Description

Active device data entry.

## Member Data Documentation

## ◆ DeviceId

xsd__string unsp__ActiveDeviceDataEntry::DeviceId

For Subscriber Devices: If the application type is Telefonica then the Service ID is returned in EID+ExtensionFormat.

For other application types the device number is presented in FQN format. For NID Devices: The NID of the device
default value[range]: NA [1..15]

## ◆ EBGId

xsd__string unsp__ActiveDeviceDataEntry::EBGId

The EBGID.

Applicable for Telefonica application type only and Subscriber device type.
default value[range]: NA [1..32]

## ◆ Monitor

xsd__boolean unsp__ActiveDeviceDataEntry::Monitor

Indicates whether this device has active monitors for the CSTA application.

## ◆ RouteRegistration

xsd__boolean unsp__ActiveDeviceDataEntry::RouteRegistration

Indicates whether this device has active Route Registrations for the CSTA application.

## ◆ Type

enum unsp__CSTADeviceType unsp__ActiveDeviceDataEntry::Type

Indicates whether this device is a Subscriber or NID.

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h