| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__ModifyOpModeRequest Struct Reference
General Utility Interfaces

Modify Operation Mode request. More...

`#include <osv-if-doc.h>`

## Public Attributes
char * | OperatorId
| Operator Id. More...
enum unsp__OpModeStatus * | NewOpMode
| Specifies the operation mode status of the node of the cluster to be modified. More...

## Detailed Description

Modify Operation Mode request.

Used by unsp__ModifyOpMode()

## Member Data Documentation

## ◆ NewOpMode

enum unsp__OpModeStatus* unsp__ModifyOpModeRequest::NewOpMode

Specifies the operation mode status of the node of the cluster to be modified.

The administrator can manually change the operation mode of a node in a cluster only if the two nodes cannot communicate with one another over the cross-channel. The Allowed 'from' states are:

- StandAlonePrimary
- StandAloneSecondary

The manual modification is allows for only the own node because there is no communication with the partner node.
required: true

## ◆ OperatorId

char* unsp__ModifyOpModeRequest::OperatorId

Operator Id.

See also
  unsp__OperatorId

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h