| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__SerialDNEntry Struct Reference

Serial DN Entry. More...

`#include <osv-if-doc.h>`

## Public Attributes
unsp__ServiceId | ServiceID
| A DN or alphanumeric SIP URI to be rung serially. More...
xsd__int * | Duration
| Period of time this entry's phone rings before the next DN in the list is dialed. More...
unsp__Enabled * | DNActive
| Indicates whether this DN is to be rung (True) or skipped (False). More...
enum unsp__SubscriberPPS * | PPSState
| Indicates whether the this entry's DN is public or private. More...
xsd__boolean * | Extension
| Indicates that the DN is an extension, or intercom dialing code (True). More...

## Detailed Description

Serial DN Entry.

## Member Data Documentation

## ◆ DNActive

unsp__Enabled* unsp__SerialDNEntry::DNActive

Indicates whether this DN is to be rung (True) or skipped (False).

required: false
default value[range]: false

## ◆ Duration

xsd__int* unsp__SerialDNEntry::Duration

Period of time this entry's phone rings before the next DN in the list is dialed.

required: true
default value[range]: 18 [1..120]

## ◆ Extension

xsd__boolean* unsp__SerialDNEntry::Extension

Indicates that the DN is an extension, or intercom dialing code (True).

If False, the number is not an extension, but a fully qualified national numbering plan formatted number.
required: false
default value[range]: false

## ◆ PPSState

enum unsp__SubscriberPPS* unsp__SerialDNEntry::PPSState

Indicates whether the this entry's DN is public or private.

required: false
default value[range]: Public

## ◆ ServiceID

unsp__ServiceId unsp__SerialDNEntry::ServiceID

A DN or alphanumeric SIP URI to be rung serially.

required: true

See also
  unsp__CFTarget

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h