| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__CfCPUD Struct Reference
Subscriber Features

Call Pickup Directed. More...

`#include <osv-if-doc.h>`

## Public Attributes
enum unsp__Subscribed | Subscribed
| Standard Subscribed enumeration. More...
unsp__Enabled * | Enabled
| Standard Enabled flag. More...
struct unsp__CfCPUD_locPres * | Local
| Local Presence flags. More...

## Detailed Description

Call Pickup Directed.

This feature allows a station user to answer a call on another telephone from their telephone. The feature is allowed for Business Group Lines and Feature Profile level (FP). The feature is applicable only to SIP subscribers with an OpenStage SIP device. Only OpenStage phones support this feature. Additionally, only calls to BGLs within the same BG can be picked up, and only a single dialog can be picked up. Call pickup directed can be used to pick up calls in the following states:

- Ringing
- Camped on (Call waiting)

MP2 command: CFCPUD [Attributes]

## Member Data Documentation

## ◆ Enabled

unsp__Enabled* unsp__CfCPUD::Enabled

Standard Enabled flag.

## ◆ Local

struct unsp__CfCPUD_locPres* unsp__CfCPUD::Local

Local Presence flags.

## ◆ Subscribed

enum unsp__Subscribed unsp__CfCPUD::Subscribed

Standard Subscribed enumeration.

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h