| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__CfCFB Struct Reference
Subscriber Features

Call Forwarding Busy Line. More...

`#include <osv-if-doc.h>`

## Public Attributes
enum unsp__Subscribed | Subscribed
| Standard Subscribed enumeration. More...
enum unsp__SubControllable * | SubActivatable
| Indicates the method by which the subscriber can activate/deactivate this feature. More...
enum unsp__SubControllable * | DestServiceIdSubControllable
| Indicates the method by which the subscriber can change the destination of Call Forwarding. More...
unsp__Enabled * | Enabled
| Standard Enabled flag. More...
unsp__ServiceId | ServiceId
| Indicates the destination number or Alphanumeric SIP URI. More...
enum unsp__CFNotifyCallingParty * | CFNotifyCallingParty
| Specifies whether and how the calling party will be notified of the forwarding. More...
xsd__boolean * | NotifySubCallFwdActive
| If set to True, the user is reminded that forwarding is currently active. More...
struct unsp__CfCFB_locPres * | Local
| Local Presence flags. More...

## Detailed Description

Call Forwarding Busy Line.

The Call Forwarding Busy Line (CFBL) feature provides the capability to redirect calls intended for the subscriber to another destination when the subscriber's station is in use.
MP2 command: CFCFB [Attributes]

## Member Data Documentation

## ◆ CFNotifyCallingParty

enum unsp__CFNotifyCallingParty* unsp__CfCFB::CFNotifyCallingParty

Specifies whether and how the calling party will be notified of the forwarding.

required: false
default value[range]: CfNotifyCallingPtyNone

## ◆ DestServiceIdSubControllable

enum unsp__SubControllable* unsp__CfCFB::DestServiceIdSubControllable

Indicates the method by which the subscriber can change the destination of Call Forwarding.

The option can be set to All only if SubActivatable is set to All
required: false
default value[range]: None

## ◆ Enabled

unsp__Enabled* unsp__CfCFB::Enabled

Standard Enabled flag.

## ◆ Local

struct unsp__CfCFB_locPres* unsp__CfCFB::Local

Local Presence flags.

## ◆ NotifySubCallFwdActive

xsd__boolean* unsp__CfCFB::NotifySubCallFwdActive

If set to True, the user is reminded that forwarding is currently active.

The notification method can be either tone or announcement, which is part of the treatment provisioning, not part of the feature provisioning..
required: false
default value[range]: false

## ◆ ServiceId

unsp__ServiceId unsp__CfCFB::ServiceId

Indicates the destination number or Alphanumeric SIP URI.

required: true, if the feature is enabled

See also
  unsp__CFTarget

## ◆ SubActivatable

enum unsp__SubControllable* unsp__CfCFB::SubActivatable

Indicates the method by which the subscriber can activate/deactivate this feature.

required: false
default value[range]: None

## ◆ Subscribed

enum unsp__Subscribed unsp__CfCFB::Subscribed

Standard Subscribed enumeration.

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h