| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__CfEpCT Struct Reference
Endpoint Profile Features

Call Transfer. More...

`#include <osv-if-doc.h>`

## Public Attributes
enum unsp__Subscribed | Subscribed
| Standard Subscribed enumeration. More...
unsp__Enabled * | Enabled
| Standard Enabled flag. More...

## Detailed Description

Call Transfer.

SIP Endpoints, configured with the endpoint profile, were restricted from invoking the call transfer feature. As an alternative, such endpoints employed the re-invite mechanism with the result that two channels were held up for the duration of the call. In an IVR or voice mail system, such a mechanism had a huge impact on performance and capacity. The call transfer mechanism is needed for Genesys and other IVRs and Xpressions. In the case of Xpressions, if the call transfer feature functionality is available, all SIP ports on XPressions could use a single SIP connection for the calls. Further, this single SIP connection could be secured by TLS. The CfEpCT feature is applicable only to endpoint profiles.
MP2 command: CFEpCT [Attributes]

## Member Data Documentation

## ◆ Enabled

unsp__Enabled* unsp__CfEpCT::Enabled

Standard Enabled flag.

## ◆ Subscribed

enum unsp__Subscribed unsp__CfEpCT::Subscribed

Standard Subscribed enumeration.

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h