| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__CfLINR Struct Reference
Subscriber Features

Last Incoming Number Redial. More...

`#include <osv-if-doc.h>`

## Public Attributes
enum unsp__Subscribed | Subscribed
| Standard Subscribed enumeration. More...

## Detailed Description

Last Incoming Number Redial.

The LINR (Last Incoming Number Redial ) feature provides subscribers the capability to perform an activation procedure that automatically sets up a call to the last incoming number. The incoming number stored can be any of the following:

- The last incoming call that alerted at the subscriber endpoint
- A call retrieved via directed call pickup or group call pickup
- A call retrieved from manual hold.

The subscriber need not know the telephone number of the last incoming call.The administrator can allow the subscriber to activate LINR for callers who have their calling identity suppressed.

OpenScape Voice places a call to the last incoming number stored and the following takes place:

- If the called party is idle: The call begins alerting normally.
- If the called party is busy: The calling subscriber hears busy tone. To camp on to the called party's station, the subscriber must enter the CCBS access code.

MP2 command: CFLINR [Attributes]

## Member Data Documentation

## ◆ Subscribed

enum unsp__Subscribed unsp__CfLINR::Subscribed

Standard Subscribed enumeration.

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h