| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__CreateMediaGatewayCircuitsRequest Class Reference
Media Server

Create Media Gateway Circuits request. More...

`#include <osv-if-doc.h>`

## Public Attributes
xsd__string | OperatorId
| Operator Id. More...
xsd__string | GatewayName
| Name of the media gateway. More...
enum unsp__CircuitAssignment | CircuitType
| Circuit type. More...
xsd__string | StartCircuitId
| Start Circuit Id. More...
xsd__string | EndCircuitId
| End Circuit Id. More...

## Detailed Description

Create Media Gateway Circuits request.

Used by unsp__createMediaGatewayCircuits()

## Member Data Documentation

## ◆ CircuitType

enum unsp__CircuitAssignment unsp__CreateMediaGatewayCircuitsRequest::CircuitType

Circuit type.

required: true
default value[range]: CircuitDoesNotExist

## ◆ EndCircuitId

xsd__string unsp__CreateMediaGatewayCircuitsRequest::EndCircuitId

End Circuit Id.

required: true
default value[range]: NA

## ◆ GatewayName

xsd__string unsp__CreateMediaGatewayCircuitsRequest::GatewayName

Name of the media gateway.

required: true
default value[range]: NA [1..63]

## ◆ OperatorId

xsd__string unsp__CreateMediaGatewayCircuitsRequest::OperatorId

Operator Id.

See also
  unsp__OperatorId

## ◆ StartCircuitId

xsd__string unsp__CreateMediaGatewayCircuitsRequest::StartCircuitId

Start Circuit Id.

required: true
default value[range]: NA

The documentation for this class was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h