| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__LPLinListEntry Struct Reference
Business Group

Entry of Lin Pool List. More...

`#include <osv-if-doc.h>`

## Public Attributes
char * | LIN
| Location Identifier Number for the subnet; used for all L2 switches discovered in this subnet. More...
char * | CallbackNumber
| Callback Number in case the Public Safety Answering Point (ie PSAP) needs to call back. More...
char * | DefaultCallbackNumber
| Default Callback Number; When PSAP is not available, the call is redirected to a default callback number. More...
xsd__boolean * | UseDefaultCallbackNumber
| Should we use Default Callback Number; If set to true, the Default Callback Number is used instead of the Callback Number . More...

## Detailed Description

Entry of Lin Pool List.

Used by unsp__LPLinList

## Member Data Documentation

## ◆ CallbackNumber

char* unsp__LPLinListEntry::CallbackNumber

Callback Number in case the Public Safety Answering Point (ie PSAP) needs to call back.

required: true
default value[range]: NA [1..25]

## ◆ DefaultCallbackNumber

char* unsp__LPLinListEntry::DefaultCallbackNumber

Default Callback Number; When PSAP is not available, the call is redirected to a default callback number.

required: false
default value[range]: NA [0..25]

## ◆ LIN

char* unsp__LPLinListEntry::LIN

Location Identifier Number for the subnet; used for all L2 switches discovered in this subnet.

required: false
default value[range]: NA [0..20]

## ◆ UseDefaultCallbackNumber

xsd__boolean* unsp__LPLinListEntry::UseDefaultCallbackNumber

Should we use Default Callback Number; If set to true, the Default Callback Number is used instead of the Callback Number .

required: false

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h