| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__Treatment Class Reference
Intercept and Treatment

Treatment data. More...

`#include <osv-if-doc.h>`

## Public Attributes
TreatmentId | TreatmentInfo
| Treatment Id data. More...
xsd__int | Cycle
| The number of times that the intercept treatment sequence is applied. More...
xsd__int | Interval
| The time that silence between cycles shall last. More...
enum unsp__TreatmentType | Type
| The type of treatment. More...
ToneInfo | Tone
| Tone data. More...
AnnounceInfo | Announce
| Announcement data. More...
xsd__int | SipReasonId
| SIP reason header that may be provided if TreatmentType is TreatmentTypeRelCall. More...
ServiceInfo * | Service
| Service data. More...

## Detailed Description

Treatment data.

## Member Data Documentation

## ◆ Announce

AnnounceInfo unsp__Treatment::Announce

Announcement data.

## ◆ Cycle

xsd__int unsp__Treatment::Cycle

The number of times that the intercept treatment sequence is applied.

This value is the same for all treatments assigned to the same intercept.
default value[range]: NA

## ◆ Interval

xsd__int unsp__Treatment::Interval

The time that silence between cycles shall last.

This value is the same for all treatments assigned to the same intercept.
default value[range]: NA

## ◆ Service

ServiceInfo* unsp__Treatment::Service

Service data.

## ◆ SipReasonId

xsd__int unsp__Treatment::SipReasonId

SIP reason header that may be provided if TreatmentType is TreatmentTypeRelCall.

## ◆ Tone

ToneInfo unsp__Treatment::Tone

Tone data.

## ◆ TreatmentInfo

TreatmentId unsp__Treatment::TreatmentInfo

Treatment Id data.

## ◆ Type

enum unsp__TreatmentType unsp__Treatment::Type

The type of treatment.

default value[range]:

The documentation for this class was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h