| Openscape Voice V10 - SOAP Interface Documentation

Public Attributes | List of all members
unsp__CSTAApplicationSOAPHeartBeat Struct Reference
CSTA Application

CSTA Application SOAP HeartBeat. More...

`#include <osv-if-doc.h>`

## Public Attributes
xsd__unsignedInt * | SOAPListenerPort
| Port that applications use when connecting to OpenScape Voice via CSTA over HTTP/SOAP. More...
xsd__unsignedInt * | HeartbeatTimer
| System Status Heartbeat timer interval value. More...
xsd__unsignedInt * | HeartbeatWatchdog
| System Status Heartbeat watchdog timer value. More...
xsd__unsignedInt * | HeartbeatRetryCount
| System Status Heartbeat retry value. More...

## Detailed Description

CSTA Application SOAP HeartBeat.

## Member Data Documentation

## ◆ HeartbeatRetryCount

xsd__unsignedInt* unsp__CSTAApplicationSOAPHeartBeat::HeartbeatRetryCount

System Status Heartbeat retry value.

required: false
default value[range]: 0 [0..5]

## ◆ HeartbeatTimer

xsd__unsignedInt* unsp__CSTAApplicationSOAPHeartBeat::HeartbeatTimer

System Status Heartbeat timer interval value.

A value of 0 disables the heartbeat function.
required: false
default value[range]: 0 [0-3600]

## ◆ HeartbeatWatchdog

xsd__unsignedInt* unsp__CSTAApplicationSOAPHeartBeat::HeartbeatWatchdog

System Status Heartbeat watchdog timer value.

required: false
default value[range]: 0 [70..360]

## ◆ SOAPListenerPort

xsd__unsignedInt* unsp__CSTAApplicationSOAPHeartBeat::SOAPListenerPort

Port that applications use when connecting to OpenScape Voice via CSTA over HTTP/SOAP.

CSTA over HTTP/SOAP uses same the IP address as CSTA over TCP.
required: false
default value[range]: 7780 [80, 1024 - 65535]

The documentation for this struct was generated from the following file:

- /home/build/gitlocal/osv_nem/submgmt/doc/osv-if-doc.h